# 3D Printed Parametric Flat Crate

This is the clean flat-pack crate release only. It contains the parametric
OpenSCAD source, A1 Mini and A1 single-plate STL files, H2S individual part
STLs, the tab-lock validation coupon, assembly media, project photos, and the
CC BY 4.0 license.

It deliberately does not include the unrelated one-piece crate project.

Start with the coupon, print at 100% without supports, and use a 0.6 mm nozzle
with PLA or PLA+ at 0.20–0.24 mm layers as a sensible baseline. The A1 Mini
full crate and coupon were physically tested; the A1 and H2S sets are
generated variants and should be coupon-tested on their target printer first.

See the OpenSCAD source for presets and the full print/assembly instructions
in the article.
